Mosfet:

RDSon represents DS Resistance in the lower part of the linear region when conducing:
    VGS > Vth and VDS < ( VGS – Vth )

It is posible to configure it as P or N channel as well as a depletion mosfet.
