Current Source:

This is a variable Current Source.

Current can be adjusted from 0V to max. current using the dial.

It can be turned On/Off with the buttton on the bottom side.

Button label shows current output value.
