Relay:

Configurable electromagnetic relay.

To adjust number of poles use "Poles" property.

It can be configured as Double or Sigle Throw using "DT" property:

DT = true  : Double Throw.
DT = false : Sigle  Throw.

You can also adjust coil resistance and trigger current.
