Led:

To simplify the circuit you can set "Gronded" property to true.
This creates a virtual connection from diode cathode to ground.
Cathode pin will dissapear deleting any wire connected to it.

Led will blink white when the maximun current is exedeed by aprox 40%.

More Info:
 http://simulide.blogspot.com/p/leds.html
